/****************************************************************/
/*  PCI-1002 DLL Driver and OCX(ActiveX) Control                */
/*  for Windows 95/98/ME                                        */
/*                                                              */
/*  Version : 3.01.00                                           */
/*  Update  : Mar-29-2006                                       */
/****************************************************************/

A. The default installation folder is 
   C:\DAQPro\PCI-1002_Win98

B. It's recommended to install the software before plug PCI-1002
   into the computer. This reduces the Windows Plug & Play procedures.
     
     1. Run the setup program to install.
     2. Power-off your computer.
     3. Plug the PCI-1002 card into the computer.
     4. Re-start the computer and finish the Windows PnP.
     
   If Windows still asking the Inf files for PnP, please specify the
   "C:\DAQPro\PCI-1002\Driver" (depends on your installation) 
   folder to finish it.

C. For more information please refer to:
   
   CD:\NAPDOS\PCI\PCI-1002\DLL_OCX\Demo    (Sample programs)
   CD:\NAPDOS\PCI\PCI-1002\Manual          (Hardware/Software manuals)
   CD:\NAPDOS\PCI\Manual                   (Related documents)
 

Note: The PCI/PIO/PISO Series Cards must set it's Information-file 
      correctlly  under Windows 9x/2000/XP/2003 before users controlling 
      or accessing these cards. For the detailed information, please 
      refer to 
      CD:\NAPDOS\PCI\Manual\PCI_ISA_PnP_Driver_Installation_in_Win9x_2K_XP.pdf

Note: The manual is written in PDF format, users may need to free 
      download the Adobe Arcobat Reader at
      http://www.adobe.com/prodindex/acrobat/readstep.html
      or
      CD:\NAPDOS\Adobe_Reader
		
