/*************************************************************************************/
/*                                                                                                        */
/*  PCI-1002 LabVIEW v85 and later Development Toolkit                         */
/*                                                                                                        */
/*  Version : 3.03                                                                                 */
/*  Update  : May 2009                                                                        */
/*  Support Card: PCI-1002L/H, PCI-1002LU/HU                                     */
/*                       PEX-1002L/H                                                            */
/*  Support OS : Windows 2000 and XP/Vista/2003/2008/7 (32/64-bit)     */
/*                                                                                                       */
/************************************************************************************/

Installation steps:

1.Install the driver for PCI-1002
 (CD:\NAPDOS\PCI\PCI-1002\DLL_OCX\Win2K_XP)

2.Power-off the PC, plug in the card and then power-on the PC.

3.Install the LabVIEW toolkit

4.Run \Diag\DIO.exe to check whether the card and driver are installed correct.

5.Refer to the demo programs and get the description of sub-vis
  from "PCI-1002_Software_Manual.pdf" in 
  CD:\NAPDOS\PCI\PCI-1002\Manual.


About the LabVIEW 8.5 toolkit:

  a. The default path to install is c:\DAQPro\pci_1002_lv85
  b. The toolkit includes demo programs, P1002.llb, kernel32.llb and this readme.txt.
 