/****************************************************************************/
/* PCI-1202 DLL Driver and OCX(ActiveX) Control    		            */
/* for Windows 2K/XP/2003/Vista 32ĦB98ĦB NT                                 */
/*                                                                 	    */
/* Version : 2.34.00                                        		    */
/* Update  : OCT-30-2008                             		            */
/*                                                                          */
/* Support : PCI-1202L, PCI-1202H, PCI-1202LU, PCI-1202HU                   */
/****************************************************************************/

A. The default installation folder is 
   system for WINDOWS 2000/XP/2003 is C:\DAQPro\PCI-1202_Win2K
   system for WINDOWS 98 is C:\DAQPro\PCI-1202_Win98
   system for WINDOWS NT is C:\DAQPro\PCI-1202_WinNT 
      
B. It's recommended to install the software before plug PCI-1202 series cards
   into the computer. This reduces the Windows Plug & Play procedures.
     
     1. Run the setup program to install.
     2. Power-off your computer.
     3. Plug the PIO-DA series cards into the computer.
     4. Re-start the computer and finish the Windows PnP.
     
   Usually, Windows 2000 will finish the PnP procedures automatically.
   If Windows still asking the Inf files for PnP, please specify the
   "C:\DAQPro\PCI-1202_Win2K\Driver" (depends on your installation) 
   folder to finish it.

   If Windows still asking the Inf files for PnP, please specify the
   "C:\DAQPro\PCI-1202_Win98\Driver" (depends on your installation) 
   folder to finish it.

C. For more information please refer to:
   
   CD:\NAPDOS\PCI\PCI-1202\Manual           (Hardware manual)
   CD:\NAPDOS\PCI\PCI-1202\DLL_OCX\Demo     (Sample programs)
   CD:\NAPDOS\PCI\Manual                  (Related documents)

Note: It will return PIODA_DriverOpenError under Windows 2000 when the 
      driver found no devices on the system.

Note: The PCI/PIO/PISO Series Cards must set it's Information-file 
      correctlly  under Windows 9x/2000/XP/2003 before users controlling 
      or accessing these cards. For the detailed information, please 
      refer to 
      CD:\NAPDOS\PCI\Manual\PCI_ISA_PnP_Driver_Installation_in_Win9x_2K_XP.pdf

Note: The manual is written in PDF format, users may need to free 
      download the Adobe Arcobat Reader at
      http://www.adobe.com/prodindex/acrobat/readstep.html
      or
      CD:\NAPDOS\Adobe_Reader

