Please Refer to .\old_new\release note.doc

/**************************************************************/
/*                                                            */
/*  PCI-1602 Development Toolkit                              */
/*  for Windows 95/98                                         */
/*                                                            */
/*  Version : 2.20.01                                         */
/*  Update  : Dec-14-2002                                     */
/*                                                            */
/*  Installation Guide of PCI-1602 Toolkit for Win95/98       */
/**************************************************************/

The READNE.TXT contains the newest information for PCI-1602.
Please reading this file before installing.

1) When plug a PCI-1602 card into your system. The Plug&Play function
   of Windows 95/98 will request you to insert a setup disk that contain the 
   setting information file(P1602.INF). 
   Please browsing into the D:\CDSETUP\[Inf] sub-directory 
   (where D: is the CD-ROM drive)

2) to run D:\CDSETUP\SETUP\SETUP.EXE to install all software for PCI-1602.
   (please enter the path according to your environment)

3) After installed, the directory tree as follows:
     [Base Directory] <-- the directory you selected to setup
	|--\Demo  
	|   |--\VB5            <-- demo code of Visual Basic 5
	|   |--\VC5            <-- demo code of Visual C++ 5
	|   |--\Delphi3        <-- demo code of Delphi 3
	|   |--\BCB3           <-- demo code of Borland C++ Builder 3
	|          
	|--\Driver <-- some device driver
	|   |--\P1602.dll      <-- dynamic linking library for PCI-180X card 
	|   |--\nappci.vxd     <-- kernel mode device driver
	|
	|--\Inf
        |   |--\NAPPCI.VXD     <-- virtual device driver
        |   |--\P1602.inf      <-- setting information file	
	|   |--\P1602.dll      <-- dynamic linking library for PCI-180X card
	|	
	|--\Manual
	|   |--\1602soft.pdf   <-- the software manual 
	|   |--\P180xHw.pdf    <-- the hardware manual for PCI-1202/1602/1800/1802
        |   |--\CallDLL.pdf    <-- describes how to call the DLL functions 
        |   |                      with VC++5.0, VB5.0, Delphi3.0 
        |   |                      and Borland C++ Builder 3.0.
        |   |--\ResCheck.pdf   <-- describes how to check the resoures 
        |                          under Windows 95/98/NT
	|
	|--\readme.txt	       <-- this file           


Note: The PCI/PIO/PISO Series Cards must setting it's Information-file 
      correctly  under Windows 95/98/2000 before users control(access) 
      these cards.  For the  detailed  informations,  please  refer to 
      Inf\PnPInstall.PDF.

Note: The manual is written in PDF format,
      the user may need to free download the Adobe Arcobat Reader at
      http://www.adobe.com/prodindex/acrobat/readstep.html 





------------------- demo1 & demo2 ---------------------------
. D/I/O, D/A, A/D polling, general test
. demo1 --> for single board, demo2 --> for two board


------------------- demo3 & demo4 ---------------------------
. A/D software-trigger and pacer-trigger demo
. demo3 --> for single board, demo4 --> for two board


------------------- demo5 & demo6 ---------------------------
. M_Function_1 demo
. demo5 --> for single board, demo6 --> for two board
------------------- demo7 & demo8 ---------------------------
. M_Function_2 demo
. demo7 --> for single board, demo8 --> for two board
------------------- demo9 & demo10 --------------------------
. M_Function_3 demo
. demo9 --> for single board, demo10 --> for two board


------------------- demo11 & demo12 -------------------------
. MagicScan function demo
. demo11 --> for single board, demo12 --> for two board


------------------- demo13 -------------------------
. Continuous capture function demo
. demo13 --> for single board


------------------- demo15 ----------------------------------
. D/I/O test for board number identification
. demo13 --> for single board, demo14 --> for two board


------------------- demo16 ----------------------------------
. Performance evaluation for single board


------------------- demo17 ----------------------------------
. MagicScan demo1 for single board, scan sequence=4->3->5
------------------- demo18 ----------------------------------
. MagicScan demo2 for single board, scan 32 channel, show 0/1/15/16/17


------------------- demo19 ----------------------------------
. A/D Calibration for single board 
Note: Each PCI-1602 Series card is already fully calibrated when shipped from the factory,
so it is usually unnecessary to calibrate the board again unless the accuracy is lost.


------------------- demo29 [BC/TC only]----------------------
. MagicScan Testing for one board
------------------- demo30 [BC/TC only]----------------------
. Pacer Triger testing for single board
------------------- demo31 [BC/TC only]----------------------
. Polling testing for single board
------------------- demo32 [BC/TC only]----------------------
. Monitoring the incoming data when continous capture
 		